LabWindows/CVI Drivers for M4K429RTx, DAS-429PCMCIA/RTx, DAS-429ExCARD/RTx, DAS-429UNET/RTx for Windows

Version 1.5   ---   21 Nov 18
- Using the EXEs as compiled under LW-CVI 2013 for use on 32bit and 64bit Windows
- Using new DLL set (RTx rev 4.1)
- Compiled projects/programs are 32bit & 64bit; in separate subfolders, with Select_XXX.bat batch files to select them

Version 1.4   ---   16 May 18
- Added Exc429RTxMs.dll & .lib to the folder PCIDLLS (rtxms.lib opens Exc429RTxMs.dll)
- Recompiled demo_rtx using LabWindows CVI 9

Version 1.3.1   ---   21 Nov 17
- Replaced rtxms.lib for VME with the correct file; added additional VME DLLs to the folder VMEDLLS
- Batch files: Changed xcopy to copy, so that running the batch files will run under Windows 10

Version 1.3   ---   06 Jul 17
- Fixed rtxms.h file (changed "borland_dll VMEVXI" to "#ifndef VMEVXI"; added typedef for uint; added include to rtxIncl.h for Irig functions in proto_rtx.h)
- Recompiled demo_rtx using LabWindows CVI 2015

Version 1.2   ---   26 Aug 15
- updated rtxms.h file to include all the newer functions in proto_rtx.h
- Installation package forces the user to select the option of which product he wishes to run:
PCI, VME, UNET. We copy the appropriate DLLs and LIB files to the target installation folder.
- Will install & run under 32bit or 64bit Windows, running 32bit LabWindows CVI
- compiled under CVI 9.0

Version 1.1   ---   07 Oct 08
- Modified the screen for Init_Module and for demo_rtx.uir to allow device number 0-255 and module number 0-7, for use on EXC-4000VME/VXI boards (requires the newly named rtxms.dll appropriate for the M4K429RTx module on EXC-4000VME/VXI boards)

Version 1.0  July 7, 2002
- Initial Release, based on DAS-429VME/VXI/RxTx for Win9x/NT 2.1
- CVI Drivers written under NI Measurement Studio 6.0.0.